| LEFT-HAND REAR WIRING
H45/DG

#### 1279
TELEVISION (TUNER)
TR4X2/NINAV2,NINAV4/RAD03,RAD07

13 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
14 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
17 | 0.5 | 34MC | HEADPHONE AUXILIARY INPUT EARTH | ?????
20 | 0.5 | 176D | TELEVISION IMAGE EARTH | ?????
22 | 0.5 | 34KV | TELEVISION CAN L SIGNAL (TUNER) | ?????
23 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
24 | 0.5 | 46BY | NAVIGATION CAN H SIGNAL 2 | ?????
1 | 0.5 | BP26 | CARPHONE PROTECTED + BATTERY FEED | ?????
2 | 0.5 | 34HU | MULTIMEDIA WAKE-UP SIGNAL | ?????
4 | 0.5 | 34MA | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
6 | 0.5 | 34MB | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
7 | 0.5 | TB46 | TELEVISION IMAGE SHIELDED CABLE | ?????
8 | 0.5 | 176C | TELEVISION + IMAGE OUTPUT + SIGNAL | ?????
10 | 0.5 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
11 | 0.5 | 34KU | TELEVISION CAN H SIGNAL (TUNER) | ?????
12 | 0.5 | 46BZ | NAVIGATION CAN L SIGNAL 2 | ?????