| CONNECTION
ANY TYPE

#### R683
REAR LEFT/LEFT-HAND TAILGATE 2
H45/DG TR4X2/NINAV2,NINAV4/RAD03,RAD07

1 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL | ?????
2 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
3 | 1.2 | 36A | REAR WIPER + CONTROL | ?????
5 | 0.85 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED | ?????
6 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
8 | 0.85 | H66P | REVERSING LIGHTS + CONTROL | ?????
9 | 0.5 | 36C | REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL | ?????