| CONNECTION
ANY TYPE

#### R450
DASHBOARD/RIGHT REAR 3
H45/DG TR4X4,TR4X2/RAD02

9 | 0.5 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | M004
10 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | M004
11 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | M004
14 | 0.3 | 70BR | RIGHT-HAND REAR WHEEL AERIAL RECEIVER EARTH | M004
15 | 0.3 | 70BQ | RIGHT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL | M004
16 | 0.3 | 26R | RIGHT HAND REAR HANDLE INFRARED SENSOR SIGNAL | M004
17 | 0.3 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2 | M004
18 | 0.3 | 26CK | PASSENGER REAR DOOR SWITCH/LOCKING SIGNAL | M004
19 | 0.3 | 26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL | M004
20 | 0.5 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL | M004
1 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | M004
2 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | M004
4 | 0.3 | 70BM | RIGHT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY | M004
5 | 0.3 | 70BP | RIGHT-HAND REAR RADIO FREQUENCY AMPLITUDE SIGNAL | M004
6 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | M004
7 | 0.3 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL | M004
8 | 0.3 | 26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL | M004