| LEFT-HAND REAR WIRING
H45/DG

#### 1838
AUDIBLE WARNING
TR4X2/RDAVAR/RAD02,RAD04,RAD05

2 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | F005E
3 | 0.5 | 80FG | CENTRAL ELECTRICAL UNIT SIGNAL CODE / UCH COMPUTER CONTROL | F005E
4 | 0.3 | 67A | HORN + CONTROL | F005E
5 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | F005E
6 | 0.3 | 64Q | FLASHER UNIT TIMER - CONTROL | F005E