| CONNECTION
ANY TYPE

#### R2
DASHBOARD/LEFT REAR CONNECTION
H45/DG FMMANU/SOP01/LVILVE/RAD02/BVA6/BVVR

1 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL | ?????
5 | 0.3 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
6 | 0.5 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL | ?????
8 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | ?????
14 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | ?????
16 | 0.5 | 85U | 4X4 SOLENOID VALVE - CONTROL | ?????
17 | 0.85 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED | ?????
18 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL | ?????
29 | 0.5 | 60EE | FRONT LEFT-HAND SEAT BELT SENSOR SIGNAL | ?????
30 | 0.5 | 13E | INTERIOR LIGHTS - CONTROL > TIMER | ?????
31 | 0.5 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL | ?????
32 | 0.5 | 85T | 4X4 SOLENOID VALVE + CONTROL | ?????