| CONNECTION
ANY TYPE

#### R12
RIGHT REAR/RIGHT-HAND REAR DOOR CONNECTION
H45/DG TR4X4,TR4X2/RAD03

2 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | F009
3 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | F009
4 | 0.85 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL | F009
5 | 0.85 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL | F009
6 | 0.3 | 26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL | F009
7 | 0.3 | 26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL | F009
8 | 0.3 | 26CK | PASSENGER REAR DOOR SWITCH/LOCKING SIGNAL | F009
10 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | F009
11 | 1.2 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
12 | 1.2 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
13 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
14 | 1.2 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
15 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | ?????
16 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
17 | 1.2 | 20AR | DEADLOCKING MOTOR CONTROL | ?????
18 | 0.3 | 26R | RIGHT HAND REAR HANDLE INFRARED SENSOR SIGNAL | ?????