24342AX119
1	0.5	87T	BOOT LID POSITION SWITCH 1 SIGNAL	?????
5	0.3	87A	LEFT HAND REAR 1st POSITION SWITCH - SIGNAL	?????
6	0.5	87H	DRIVER'S 1st POSITION SWITCH - SIGNAL	?????
8	0.3	LP	PROTECTED + SIDE LIGHT FEED	?????
14	0.5	BPT	PROTECTED + BATTERY FEED TIMER	?????
16	0.5	85U	4X4 SOLENOID VALVE - CONTROL	?????
17	0.85	20S	TAILGATE MOTOR OPENING AUTHORISED FEED	?????
18	0.5	20G	TAILGATE MOTOR OPEN CONTROL 	?????
29	0.5	60EE	FRONT LEFT-HAND SEAT BELT SENSOR SIGNAL	?????
30	0.5	13E	INTERIOR LIGHTS - CONTROL > TIMER	?????
31	0.5	64C	LEFT HAND TURN SIGNAL LIGHTS CONTROL	?????
32	0.5	85T	4X4 SOLENOID VALVE + CONTROL	?????
