24341JY04A
20	0.5	38U	RHEOSTAT CURSOR	M049
22	0.5	CANL	DIAGNOSTIC CAN L SIGNAL 	M049
23	0.5	28A	OIL PRESSURE WARNING LIGHT - CONTROL	M049
24	0.5	26BM	OIL PRESSURE WARNING LIGHT/ALTERNATOR CHARGING INDICATOR LIGHT CONTROL	M049
1	0.5	26Z	AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL	M049
2	0.5	AP11	PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE	M049
3	0.5	H66P	REVERSING LIGHTS + CONTROL	M049
4	0.5	AP4	PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE	M049
5	0.5	3DV	AIRFLOW SENSOR + SIGNAL	M049
6	0.5	3ABQ	AIR FLOW TEMPERATURE SIGNAL	M049
7	0.5	BP42	PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER	M049
8	0.5	BP42	PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER	M049
9	0.5	CANH	DIAGNOSTIC CAN H SIGNAL 	M049
10	0.5	BPA4	+ BATTERY HORN PROTECTED FEED	M049
15	0.5	AP4	PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE	M049
16	0.5	3DW	AIRFLOW SENSOR - SIGNAL	M049
18	0.5	38Y	REFRIGERANT GAS PRESSURE SENSOR +	M049
19	0.5	38X	REFRIGERANT GAS PRESSURE SENSOR SIGNAL	M049
