| CONNECTION
ANY TYPE

#### R38
DASHBOARD/LEFT-HAND ROOF CONNECTION
H45/DD FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/RAD03/BVM6

1 | 0.5 | 52K | CERAMIC SUN ROOF OPENING/CLOSING CONTROL 1 | M049
2 | 0.5 | 52L | SUN ROOF OPENING/CLOSING CONTROL 2 | M049
3 | 0.5 | BP6 | PROTECTED + BATTERY FEED > INTERIOR LIGHT | M049
4 | 0.5 | 80FG | CENTRAL ELECTRICAL UNIT SIGNAL CODE / UCH COMPUTER CONTROL | M049
5 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | M049
6 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | M049
7 | 0.5 | 85AB | INSTRUMENT PANEL/RIDE HEIGHT SENSOR (COMPASS) SERIES CONNECTION EARTH | M049
8 | 0.5 | 85AA | INSTRUMENT PANEL/RIDE HEIGHT SENSOR (COMPASS) SERIES CONNECTION + SIGNAL | M049
11 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | M049
12 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | M049
13 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M049
18 | 0.5 | 14S | RAIN SENSOR SERIAL LINE SIGNAL | M049
19 | 0.5 | AP43 | PROTECED + AFTER IGNITION FUSE | M049