| CONNECTION
ANY TYPE

#### R67
FRONT OF ENGINE/ENGINE CONNECTION
H45/BVVR/2TR DD/TR4X4/ASRES2/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 0.5 | 26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL | M049
2 | 0.5 | AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE | M049
3 | 0.5 | H66P | REVERSING LIGHTS + CONTROL | M049
4 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | M049
5 | 0.5 | 3DV | AIRFLOW SENSOR + SIGNAL | M049
6 | 0.5 | 3DW | AIRFLOW SENSOR - SIGNAL | M049
7 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | M049
8 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | M049
9 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | M049
10 | 0.5 | BPA4 | + BATTERY HORN PROTECTED FEED | M049
11 | 0.85 | AP28 | PROTECTED + AFTER IGNITION FUSE COOLING FAN ASSEMBLY | M049
15 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | M049
16 | 0.5 | 3DU | AIRFLOW SENSOR - | M049
18 | 0.5 | 38Y | REFRIGERANT GAS PRESSURE SENSOR + | M049
19 | 0.5 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL | M049
20 | 0.5 | 38U | RHEOSTAT CURSOR | M049
21 | 0.5 | 3NA | IMPACT SENSOR IGNITION COIL + > FUEL PUMP RELAY | M049
22 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | M049
23 | 0.5 | 28A | OIL PRESSURE WARNING LIGHT - CONTROL | M049
24 | 0.5 | 26BM | OIL PRESSURE WARNING LIGHT/ALTERNATOR CHARGING INDICATOR LIGHT CONTROL | M049