| CONNECTION
ANY TYPE

#### R3
DASHBOARD/DRIVER'S DOOR CONNECTION
H45/DG RET03/LVILVI/RAD01,RAD02,RAD04,RAD05

3 | 0.3 | 26CE | DRIVER'S DOOR SWITCH/LOCKING SIGNAL | M049
4 | 0.3 | 26AB | KEYLESS VEHICLE DRIVER'S SIDE FRONT DOOR EXTERNAL AERIAL B SIGNAL | M049
5 | 0.3 | 26AA | KEYLESS VEHICLE DRIVER'S FRONT DOOR EXTERNAL AERIAL A SIGNAL | M049
8 | 0.5 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL | M049
9 | 0.5 | 40E | REAR VIEW MIRROR MOTOR COMMON | M049
10 | 0.5 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL | M049
11 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO | M049
14 | 0.3 | 26T | DRIVER'S HANDLE INFRARED SENSOR SIGNAL | M049
15 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | M049
16 | 0.5 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL | M049
17 | 0.5 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL | M049
19 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | M049
20 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | M049
21 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M049
22 | 0.5 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL | M049
23 | 0.5 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL | M049
24 | 0.5 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL | M049