| DASHBOARD WIRING
H45/DG

#### 261
RADIO
FMMANU/SOP01/LVILVE/RAD04/BVM6

B8 | 0.5 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL | CT2F
B1 | 0.5 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL | CT2F
B2 | 0.5 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL | CT2F
A3 | 0.5 | 107E | RADIO SOUND CUT-OFF SIGNAL FOR TELEPHONE | CT2F
B3 | 0.5 | 34JK | RIGHT-HAND AUDIO + SIGNAL | CT2F
A4 | 0.85 | BP26 | CARPHONE PROTECTED + BATTERY FEED | CT2F
B4 | 0.5 | 34JL | RIGHT-HAND AUDIO - SIGNAL | CT2F
B5 | 0.5 | 34JM | LEFT-HAND AUDIO + SIGNAL | CT2F
B6 | 0.5 | 34JP | LEFT-HAND AUDIO - SIGNAL | CT2F
B7 | 0.5 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL | CT2F
A8 | 0.85 | MT | RADIO ELECTRICAL EARTH | CT2F