24341AX119
2	0.3	26AR	KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH	M004
3	0.3	26AV	KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 1	M004
4	0.3	26CJ	DRIVER'S REAR DOOR SWITCH/LOCKING SIGNAL	M004
5	0.5	87A	LEFT HAND REAR 1st POSITION SWITCH - SIGNAL	M004
6	0.5	87H	DRIVER'S 1st POSITION SWITCH - SIGNAL	M004
7	0.3	26S	DRIVER'S SIDE REAR HANDLE INFRARED SENSOR SIGNAL	M004
8	0.3	LP	PROTECTED + SIDE LIGHT FEED	M004
11	0.3	70BS	LEFT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY	M004
12	0.3	70BT	LEFT-HAND REAR WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL	M004
14	0.5	BPT	PROTECTED + BATTERY FEED TIMER	M004
17	0.85	20S	TAILGATE MOTOR OPENING AUTHORISED FEED	?????
18	0.5	20G	TAILGATE MOTOR OPEN CONTROL 	M004
19	0.3	26AW	KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 2	M004
20	0.3	26AH	KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL B SIGNAL	M004
21	0.3	26AG	KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL A SIGNAL	M004
22	0.3	MZS	LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT	M004
24	0.3	26P	DOOR HANDLE INFRARED SENSOR +	M004
27	0.3	70BV	LEFT-HAND REAR WHEEL AERIAL RECEIVER EARTH	M004
28	0.3	70BU	LEFT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL	M004
29	0.5	60ES	FRONT RIGHT-HAND PRESENCE / POSITION EARTH	M004
30	0.5	13E	INTERIOR LIGHTS - CONTROL > TIMER	M004
31	0.5	64C	LEFT HAND TURN SIGNAL LIGHTS CONTROL	M004
1	0.5	87T	BOOT LID POSITION SWITCH 1 SIGNAL	M004
