24342AR443
1	0.5	115A	OIL TEMPERATURE SENSOR - SIGNAL	?????
2	0.5	32B	OIL LEVEL SENSOR SIGNAL 1 	?????
3	0.85	AP17	PROTECTED + AFTER IGNITION, INJECTION SIMULATOR FUSE	?????
4	1.2	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
5	0.5	85G	4X4 CLUTCH RELAY CONTROL	?????
6	0.5	3AA	INJECTION LOCKING RELAY COIL - CONTROL	?????
7	0.5	CANH	DIAGNOSTIC CAN H SIGNAL 	?????
8	1.2	AP15	PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE	?????
9	1.2	3AKD	BYPASS SOLENOID VALVE - CONTROL (HYDROCARBON REDUCTION SYSTEM)	?????
10	1.2	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
11	1.2	3BS	IGNITION COIL CONTROL	?????
12	0.85	3FB	INJECTION + > PROTECTIVE RELAY	?????
14	1.2	85D	4X4 TORQUE CONTROL	?????
15	0.85	38K	AIR CONDITIONING CUT-OFF CONTROL > PETROL-DIESEL COMPUTER	?????
16	0.5	CANL	DIAGNOSTIC CAN L SIGNAL 	?????
