| CONNECTION
ANY TYPE

#### R374
REAR LEFT-HAND WIRING / FRONT WIRING HARNESS CONNECTION
H45/BVM6/M9R DG/TR4X2/SSESP/NINAV1,NINAV2/RAD01,RAD02,RAD03

4 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL | F049
5 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL | F049
13 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR + | F049
14 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR + | F049
15 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | F049
16 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | F049