| CONNECTION
ANY TYPE

#### R2
DASHBOARD/LEFT REAR CONNECTION
H45/DG TR4X2/SOP01/RAD02,RAD04,RAD05

1 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL | M004
5 | 0.5 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL | M004
6 | 0.5 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL | M004
14 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M004
17 | 0.85 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED | ?????
18 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL | M004
29 | 0.5 | 60EE | FRONT LEFT-HAND SEAT BELT SENSOR SIGNAL | M004
30 | 0.5 | 13E | INTERIOR LIGHTS - CONTROL > TIMER | M004
31 | 0.5 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL | M004