| ENGINE WIRING
M9R/BVA6

#### 119
AUTOMATIC TRANSMISSION COMPUTER
TR4X2/CA01,CA02/M9R833

F3 | 0.5 | 5HN | SENSOR EARTH | ?????
G3 | 0.5 | 5LM | MODULATION SOLENOID VALVE SWITCH 4 SIGNAL | ?????
H3 | 0.5 | 5CZ | SHIFT SOLENOID VALVE SWITCH 1 SIGNAL | ?????
K3 | 0.5 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
M3 | 0.5 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
A4 | 0.5 | H66P | REVERSING LIGHTS + CONTROL | ?????
B4 | 0.5 | 5DH | MULTIFUNCTION SWITCH SIGNAL 3 | ?????
C4 | 0.5 | 5DJ | MULTIFUNCTION SWITCH SIGNAL 4 | ?????
M4 | 0.85 | 5LW | - COMMON SOLENOID VALVE | ?????
A1 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
B1 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
C1 | 0.5 | 5DA | GEARBOX INPUT SPEED SENSOR + SIGNAL | ?????
D1 | 0.5 | 5T | GEARBOX OUTPUT SPEED SENSOR + | ?????
E1 | 0.5 | 5HH | STEPPER MOTOR COIL A CONTROL | ?????
F1 | 0.5 | 5HK | STEPPER MOTOR COIL B CONTROL | ?????
G1 | 0.5 | 5DL | MODULATING SOLENOID VALVE 3 | ?????
H1 | 0.5 | 5Q | MODULATING SOLENOID VALVE 1 | ?????
J1 | 0.5 | 5R | MODULATING SOLENOID VALVE 2 | ?????
K1 | 0.5 | 5HG | LOCKING ON/OFF SELECTION SOLENOID VALVE CONTROL | ?????
L1 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | ?????
M1 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | ?????
C2 | 0.5 | 5HN | SENSOR EARTH | ?????
D2 | 0.5 | 5TA | GEARBOX OUTPUT SPEED SENSOR - | ?????
J2 | 0.5 | 5HM | STEPPER MOTOR COIL D CONTROL | ?????
K2 | 0.5 | 5HL | STEPPER MOTOR COIL C CONTROL | ?????
L2 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | ?????
M2 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | ?????
A3 | 0.5 | 5DF | MULTIFUNCTION SWITCH SIGNAL 1 | ?????
B3 | 0.5 | 5BY | GEARBOX OIL TEMPERATURE - | ?????
C3 | 0.5 | 5BZ | GEARBOX OIL TEMPERATURE + | ?????
D3 | 0.5 | 5KY | SHIFT SOLENOID VALVE SWITCH 2 SIGNAL | ?????
E3 | 0.5 | 5LH | MODULATION SOLENOID VALVE SWITCH 1 SIGNAL | ?????