| CONNECTION
ANY TYPE

#### R468
ENGINE WIRING / FRONT WIRING CONNECTION 2
H45/BVM6/M9R DG/TR4X4/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 0.5 | 115A | OIL TEMPERATURE SENSOR - SIGNAL | ?????
2 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | ?????
3 | 0.5 | 3TG | PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR SIGNAL | ?????
4 | 0.85 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
5 | 0.5 | 3VH | + TURBOCHARGER BEARING COOLANT PUMP | ?????
6 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL | ?????
7 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
8 | 2.0 | 3FB2 | INJECTION + > PROTECTIVE RELAY | ?????
9 | 2.0 | 3FB1 | INJECTION + > PROTECTIVE RELAY | ?????
10 | 0.5 | 3XU | -PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR | ?????
13 | 0.5 | 3MG | TURBO PRESSURE SOLENOID VALVE - CONTROL | ?????
14 | 0.5 | 3AAZ | WATER PUMP RELAY/FUEL PRESSURE ADJUSTMENT- CONTROL | ?????
15 | 0.85 | 38K | AIR CONDITIONING CUT-OFF CONTROL > PETROL-DIESEL COMPUTER | ?????
16 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????