| CONNECTION
ANY TYPE

#### R449
DASHBOARD/RIGHT REAR 2
H45/DG TR4X4,TR4X2/NINAV2

1 | 0.5 | 79FB | HEATED SEAT WARNING LIGHT CONTROL, HIGH POSITION | M004
2 | 0.5 | 79FA | HEATED SEAT WARNING LIGHT CONTROL, LOW POSITION | M004
3 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M004
4 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | M004
6 | 0.5 | TB45 | RADIO SOCKET AUXILIARY SOCKET INPUT SHIELDED CABLE | M004
7 | 0.5 | 4CZB | CLUSTER SENSOR SERIES CONNECTION - SIGNAL | M004
8 | 0.5 | 4CZ | YAW SENSOR + (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | M004
10 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | M004
11 | 0.5 | 9P | PROTECTED REAR FOG LIGHTS + CONTROL | M004
12 | 0.5 | 34HU | MULTIMEDIA WAKE-UP SIGNAL | M004
13 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | M004
14 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | M004
16 | 0.5 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | M004
17 | 0.5 | 4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | M004
18 | 0.5 | 4CZA | CLUSTER SENSOR SERIES CONNECTION + SIGNAL | M004
19 | 0.5 | 41B | FUEL LEVEL - | M004
20 | 0.5 | 41A | FUEL LEVEL SENDER + SIGNAL | M004