| DASHBOARD WIRING
H45/DG

#### 476
INTEGRATED DRIVESHAFT COMPUTER
FMMANU/SOP01/LVILVE/RAD04/BVM6

1 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
2 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | ?????
3 | 0.5 | 4LA | ELECTRONIC STABILITY CONTROL/4X4 COMPUTER LIN SIGNAL | ?????
4 | 0.3 | 85V | 4X4 AUTOMATIC MODE SIGNAL | ?????
7 | 0.5 | 85U | 4X4 SOLENOID VALVE - CONTROL | ?????
8 | 0.5 | 85T | 4X4 SOLENOID VALVE + CONTROL | ?????
9 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
11 | 0.3 | 85Q | 4X4 MODE SIGNAL | ?????
13 | 0.3 | 85R | 4X2 MODE SIGNAL | ?????
14 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
15 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
16 | 0.5 | AP1C | PROTECTED + AFTER IGNITION FEED/4X4 COMPUTER | ?????