| DASHBOARD WIRING
H45/DG

#### 225
DIAGNOSTIC SOCKET
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD05/BVM6

4 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
5 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
6 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
6 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
8 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | ?????
8 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | ?????
12 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
13 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
14 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
14 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
15 | 0.5 | HK | DIAGNOSTIC SIGNAL K | ?????
15 | 0.5 | HK | DIAGNOSTIC SIGNAL K | ?????
16 | 0.3 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????