| LEFT-HAND REAR WIRING
H45/DD

#### 1917
AUDIO AMPLIFIER
TR4X4/NINAV2/RAD03

1 | 0.5 | 34EJ | SPEAKER - SIGNAL (BASS SECTION) | F047
2 | 0.85 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL | F048
3 | 2.0 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
4 | 2.0 | BP1H | PROTECTED + BATTERY FEED/MULTIMEDIA | ?????
5 | 0.85 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL | F047
6 | 0.5 | 34EH | SPEAKER + SIGNAL (BASS SECTION) | F047
7 | 0.85 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL | F047
8 | 0.5 | 34EW | RIGHT-HAND FRONT SPEAKER - SIGNAL (TWEETER) | F047
9 | 0.5 | 34EV | RIGHT-HAND FRONT SPEAKER + SIGNAL (TWEETER) | F047
10 | 0.85 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL | F047
11 | 0.85 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL | F047
12 | 0.85 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL | F047
13 | 0.85 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL | F047
14 | 0.85 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL | F047