| LEFT-HAND REAR WIRING
H45/DG

#### 260
PASSENGER COMPARTMENT FUSE BOX AND RELAY
TR4X4/NINAV2,NINAV4/RAD03,RAD07

4 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
5 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
10 | 1.2 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????
11 | 1.2 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????
12 | 2.0 | BP1H | PROTECTED + BATTERY FEED/MULTIMEDIA | ?????