| CONNECTION
ANY TYPE

#### R449
DASHBOARD/RIGHT REAR 2
H45/DG TR4X4/RAD02/NISEUC,NISEXP

1 | 0.5 | 79FB | HEATED SEAT WARNING LIGHT CONTROL, HIGH POSITION | M004
2 | 0.5 | 79FA | HEATED SEAT WARNING LIGHT CONTROL, LOW POSITION | M004
3 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M004
4 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | M004
7 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | M004
8 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | M004
10 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | M004
11 | 0.5 | 9P | PROTECTED REAR FOG LIGHTS + CONTROL | M004
13 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | M004
14 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | M004
15 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | M004
17 | 0.5 | 4DS | - YAW SENSOR | M004
18 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | M004
19 | 0.5 | 41B | FUEL LEVEL - | M004
20 | 0.5 | 41A | FUEL LEVEL SENDER + SIGNAL | M004