| CONNECTION
ANY TYPE

#### R450
DASHBOARD/RIGHT REAR 3
H45/DG FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD03/BVA6/BVVR

1 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
2 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
2 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
3 | 0.5 | 34MA | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
6 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | ?????
7 | 0.3 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL | ?????
8 | 0.3 | 26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL | ?????
9 | 0.3 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
10 | 0.5 | 60DS | PASSENGER AIR BAG INHIBITOR KEY SIGNAL | ?????
11 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
12 | 0.5 | 34MC | HEADPHONE AUXILIARY INPUT EARTH | ?????
13 | 0.5 | 34MB | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
16 | 0.3 | 26R | RIGHT HAND REAR HANDLE INFRARED SENSOR SIGNAL | ?????
17 | 0.3 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2 | ?????
18 | 0.3 | 26CK | PASSENGER REAR DOOR SWITCH/LOCKING SIGNAL | ?????
19 | 0.3 | 26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL | ?????
20 | 0.3 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL | ?????