| DRIVER'S DOOR WIRING
H45/DG

#### 134
ELECTRIC REAR-VIEW MIRROR CONTROL
RET03/LVILVE/RAD01,RAD02,RAD04,RAD05

1 | 0.5 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL | ?????
3 | 0.5 | 40E | REAR VIEW MIRROR MOTOR COMMON | ?????
4 | 0.5 | 40AA | REAR-VIEW MIRROR EARTH > REAR VIEW MIRROR ANTI-RETURN DIODE | ?????
5 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO | ?????
6 | 0.5 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL | ?????
7 | 0.5 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL | ?????
8 | 0.5 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL | ?????
9 | 0.5 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL | ?????
10 | 0.5 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL | ?????