| DASHBOARD WIRING
H45/DD

#### 1088
STEERING COLUMN ELECTRIC LOCK
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/NINAV2/BVM6

1 | 0.5 | APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST | ?????
2 | 0.3 | 26LA | PASSENGER COMPARTMENT COMMUNICATION SIGNAL/COLUMN LOCK | ?????
3 | 0.3 | 26LB | COLUMN STATUS SIGNAL 1 | ?????
5 | 0.3 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
6 | 0.3 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
7 | 0.3 | 26I | + STEERING COLUMN LOCK | ?????
8 | 0.3 | 26LC | COLUMN STATUS SIGNAL 2 | ?????