| CONNECTION
ANY TYPE

#### R449
DASHBOARD/RIGHT REAR 2
H45/DD FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/RAD01,RAD02/BVM6

3 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | ?????
4 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
7 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | ?????
7 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | ?????
8 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | ?????
8 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | ?????
10 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | ?????
11 | 0.5 | 9P | PROTECTED REAR FOG LIGHTS + CONTROL | ?????
13 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | ?????
14 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
15 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | ?????
16 | 0.5 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
17 | 0.5 | 4DS | - YAW SENSOR | ?????
17 | 0.5 | 4DS | - YAW SENSOR | ?????
18 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | ?????
18 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | ?????
19 | 0.5 | 41B | FUEL LEVEL - | ?????
20 | 0.5 | 41A | FUEL LEVEL SENDER + SIGNAL | ?????