| RIGHT-HAND REAR WIRING
H45/DD

#### 260
PASSENGER COMPARTMENT FUSE BOX AND RELAY
TR4X4/RAD02

2 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
3 | 1.2 | SP4A | ACCESSORIES SOCKET 2 PROTECTED + ACCESSORIES FEED | ?????
4 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
5 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
10 | 1.2 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????
11 | 1.2 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????