| CONNECTION
ANY TYPE

#### R2
DASHBOARD/LEFT REAR CONNECTION
H45/DD TR4X4/RAD02,RAD04,RAD05

1 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL | M004
2 | 0.3 | 26AR | KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH | M004
3 | 0.3 | 26AV | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 1 | M004
4 | 0.3 | 26CJ | DRIVER'S REAR DOOR SWITCH/LOCKING SIGNAL | M004
5 | 0.5 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL | M004
6 | 0.5 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL | M004
7 | 0.3 | 26S | DRIVER'S SIDE REAR HANDLE INFRARED SENSOR SIGNAL | M004
8 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | M004
11 | 0.3 | 70BS | LEFT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY | M004
12 | 0.3 | 70BT | LEFT-HAND REAR WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL | M004
14 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M004
16 | 0.5 | 85U | 4X4 SOLENOID VALVE - CONTROL | M004
17 | 0.85 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED | ?????
18 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL | M004
19 | 0.3 | 26AW | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 2 | M004
20 | 0.3 | 26AH | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL B SIGNAL | M004
21 | 0.3 | 26AG | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL A SIGNAL | M004
22 | 0.3 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | M004
24 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | M004
27 | 0.3 | 70BV | LEFT-HAND REAR WHEEL AERIAL RECEIVER EARTH | M004
28 | 0.3 | 70BU | LEFT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL | M004
29 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | M004
30 | 0.5 | 13E | INTERIOR LIGHTS - CONTROL > TIMER | M004
31 | 0.5 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL | M004
32 | 0.5 | 85T | 4X4 SOLENOID VALVE + CONTROL | M004