| FRONT WIRING
H45/BVM6/2TR

#### 120
INJECTION COMPUTER
DD/TR4X4/SSESP/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

A1 | 0.5 | 3LS | LOAD POTENTIOMETER 1 + SIGNAL | ?????
B1 | 0.5 | 86G | CRUISE CONTROL PROGRAMMING CONTROL | ?????
D1 | 0.85 | AP17 | PROTECTED + AFTER IGNITION, INJECTION SIMULATOR FUSE | ?????
E1 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
G1 | 1.2 | 3FB | INJECTION + > PROTECTIVE RELAY | ?????
A2 | 0.5 | 3LW | LOAD POTENTIOMETER 2 + SIGNAL | ?????
C2 | 0.5 | 86V | CLUTCH POSITION SENSOR SIGNAL | ?????
E2 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
F2 | 0.5 | 26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL | ?????
G2 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
H2 | 0.5 | 65Q | STOP SWITCH SIGNAL 2 | ?????
A3 | 0.5 | 3LR | + LOAD POTENTIOMETER 1 | ?????
B3 | 0.5 | 3LU | + LOAD POTENTIOMETER 2 | ?????
E3 | 0.3 | 3PD | SPEED LIMITER ON/OFF CONTROL | ?????
F3 | 0.3 | 3FX | CRUISE CONTROL ON>OFF - CONTROL | ?????
G3 | 1.2 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
H3 | 1.2 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
A4 | 0.5 | 3LV | - LOAD POTENTIOMETER 2 | ?????
B4 | 0.5 | HK | DIAGNOSTIC SIGNAL K | ?????
C4 | 0.5 | 86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL | ?????
E4 | 0.5 | 3LT | - LOAD POTENTIOMETER 1 | ?????
G4 | 1.2 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
H4 | 1.2 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????