| FRONT WIRING
H45/BVA6/M9R

#### 1068
ADDITIONAL HEATING RELAY 2
DG/TR4X4/ASRES2/NINAV4/RAD04,RAD05,RAD07

1 | 3.0 | BP91 | PROTECTED + BATTERY FEED ADDITIONAL HEATER FUSE | ?????
2 | 0.5 | 38JV | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 2PASSENGER | ?????
3 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
4 | 3.0 | 38LM | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL / RELAY 2 | ?????