| CONNECTION
ANY TYPE

#### R450
DASHBOARD/RIGHT REAR 3
H45/DD FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/NINAV1/BVM6

2 | 0.5 | 60EH | FRONT RIGHT-HAND SEAT BELT SWITCH SIGNAL | ?????
4 | 0.3 | 70BM | RIGHT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY | ?????
5 | 0.3 | 70BP | RIGHT-HAND REAR RADIO FREQUENCY AMPLITUDE SIGNAL | ?????
9 | 0.3 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
14 | 0.3 | 70BR | RIGHT-HAND REAR WHEEL AERIAL RECEIVER EARTH | ?????
15 | 0.3 | 70BQ | RIGHT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL | ?????
20 | 0.3 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL | ?????