24342AR443
1	0.5	115A	OIL TEMPERATURE SENSOR - SIGNAL	?????
2	0.5	32B	OIL LEVEL SENSOR SIGNAL 1 	?????
3	0.5	3TG	PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR SIGNAL	?????
4	0.85	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
5	0.5	3VH	+ TURBOCHARGER BEARING COOLANT PUMP	?????
6	0.5	3AA	INJECTION LOCKING RELAY COIL - CONTROL	?????
7	0.5	CANH	DIAGNOSTIC CAN H SIGNAL 	?????
8	2.0	3FB2	INJECTION + > PROTECTIVE RELAY	?????
9	2.0	3FB1	INJECTION + > PROTECTIVE RELAY	?????
10	0.5	3XU	-PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR	?????
13	0.5	3MG	TURBO PRESSURE SOLENOID VALVE - CONTROL	?????
14	0.5	3AAZ	WATER PUMP RELAY/FUEL PRESSURE ADJUSTMENT- CONTROL	?????
16	0.5	CANL	DIAGNOSTIC CAN L SIGNAL 	?????
