| FRONT WIRING
H45/BVA6/M9R

#### 260
PASSENGER COMPARTMENT FUSE BOX AND RELAY
DD/TR4X4/ASRES2/LADECH/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

2 | 0.5 | 65G | BRAKE LIGHT CONTROL > RELAY | ?????
4 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
4 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
6 | 0.3 | 38FC | PASSENGER COMPARTMENT FAN CONTROL > RELAY | ?????
8 | 0.5 | BPA7 | BRAKE LIGHTS + BATTERY PROTECTED | ?????
14 | 2.0 | BP1Q | PROTECTED + BATTERY FEED/PASSENGER COMPARTMENT STARTING AND AFTER IGNITION | ?????
15 | 0.5 | AP1C | PROTECTED + AFTER IGNITION FEED/4X4 COMPUTER | ?????