| LEFT-HAND TAILGATE WIRING
H45

#### 1578
SUNROOF MOTOR
DD/TOELEF/SOP03

1 | 0.5 | 52L | SUN ROOF OPENING/CLOSING CONTROL 2 | CL1Y
3 | 0.5 | 52AJ | REAR DOORS CLOSING CONTROL | CL1Y
5 | 0.5 | 52K | CERAMIC SUN ROOF OPENING/CLOSING CONTROL 1 | CL1Y
7 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | CL1Y
8 | 0.3 | H47 | VEHICLE SPEED > SECONDARY SPEED SIGNAL | CL1Y
9 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | CL1Y
10 | 1.2 | MZU | ELECTRIC EARTH ARRANGEMENT, REAR LEFT AND TAILGATE | CL1Y