24342AR422
1	2.0	AP45	+ AFTER IGNITION FEED PROTECTED BY FUSE FOR PASSENGER COMPARTMENT FUNCTIONS	?????
3	0.5	65A	BRAKE LIGHTS + CONTROL	?????
4	0.3	15M	HEATED REAR SCREEN RELAY  - CONTROL 	?????
5	0.3	SP16	PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY	?????
6	0.5	BP10	PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET	?????
7	0.85	SP4G	CIGARETTE LIGHTER PROTECTED + ACCESSORIES FEED	?????
8	0.5	LP	PROTECTED + SIDE LIGHT FEED	?????
9	0.3	BPA7	BRAKE LIGHTS + BATTERY PROTECTED	?????
10	2.0	BP1H	PROTECTED + BATTERY FEED/MULTIMEDIA	?????
