| DRIVER'S DOOR WIRING
H45/DG

#### 203
DRIVER'S WINDOW MOTOR
RET03/LVILVI/NINAV2/RAD03,RAD07

5 | 0.5 | 21E | ONE-TOUCH ELECTRIC WINDOW NORMAL DOWN - CONTROL | F005E
6 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | F005E
7 | 0.5 | 21C | ONE-TOUCH ELECTRIC WINDOW NORMAL UP - CONTROL | F005E
9 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
11 | 0.5 | 21AA | DRIVER ELECTRIC WINDOW RAISE/LOWER CONTROL | F005E
13 | 1.2 | 21ZA | WINDOW WINDER THERMAL PROTECTION SIGNAL 1 | C426E
14 | 1.2 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | C426E