| FRONT WIRING
H45/BVA6/M9R

#### 1337
SWITCHING PROTECTION UNIT
DG/TR4X4/ASRES2/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03,RAD04,RAD05,RAD07

1 | 0.5 | APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST | ?????
2 | 2.0 | 3FB2 | INJECTION + > PROTECTIVE RELAY | ?????
6 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL | ?????
7 | 2.0 | 3FB1 | INJECTION + > PROTECTIVE RELAY | ?????