| DASHBOARD WIRING
H45/DD

#### 478
4X4 ACTIVATION SWITCH
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/NINAV2/BVM6

1 | 0.3 | 85R | 4X2 MODE SIGNAL | F009
2 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | F009
3 | 0.3 | 85Q | 4X4 MODE SIGNAL | F009
4 | 0.3 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | F009
5 | 0.3 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | F009
6 | 0.3 | 85V | 4X4 AUTOMATIC MODE SIGNAL | F009