| CONNECTION
ANY TYPE

#### R468
ENGINE WIRING / FRONT WIRING CONNECTION 2
2TR/BVM6 TR4X2,TR4X4/CA01,CA02/2TR700

1 | 0.5 | 115A | OIL TEMPERATURE SENSOR - SIGNAL | ?????
2 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | ?????
3 | 0.85 | AP17 | PROTECTED + AFTER IGNITION, INJECTION SIMULATOR FUSE | ?????
4 | 1.2 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
5 | 0.5 | 85G | 4X4 CLUTCH RELAY CONTROL | ?????
6 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL | ?????
7 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
8 | 1.2 | AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE | ?????
9 | 1.2 | 3AKD | BYPASS SOLENOID VALVE - CONTROL (HYDROCARBON REDUCTION SYSTEM) | ?????
10 | 1.2 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
11 | 1.2 | 3BS | IGNITION COIL CONTROL | ?????
12 | 0.85 | 3FB | INJECTION + > PROTECTIVE RELAY | ?????
14 | 1.2 | 85D | 4X4 TORQUE CONTROL | ?????
15 | 0.85 | 38K | AIR CONDITIONING CUT-OFF CONTROL > PETROL-DIESEL COMPUTER | ?????
16 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????