| CONNECTION
ANY TYPE

#### R450
DASHBOARD/RIGHT REAR 3
H45/DG FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD05/BVM6

1 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
2 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
3 | 0.5 | 34MA | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
4 | 0.3 | 70BM | RIGHT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY | ?????
5 | 0.3 | 70BP | RIGHT-HAND REAR RADIO FREQUENCY AMPLITUDE SIGNAL | ?????
7 | 0.3 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL | ?????
9 | 0.3 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
10 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
11 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
12 | 0.5 | 34MC | HEADPHONE AUXILIARY INPUT EARTH | ?????
13 | 0.5 | 34MB | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
14 | 0.3 | 70BR | RIGHT-HAND REAR WHEEL AERIAL RECEIVER EARTH | ?????
15 | 0.3 | 70BQ | RIGHT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL | ?????
17 | 0.3 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2 | ?????
20 | 0.3 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL | ?????