| FRONT WIRING
H45/BVA6/M9R

#### 1337
SWITCHING PROTECTION UNIT
DG/TR4X4/ASRES2/NINAV4/RAD04,RAD05,RAD07

1 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
2 | 0.3 | 80A | BONNET SWITCH - SIGNAL | ?????
3 | 0.5 | 28A | OIL PRESSURE WARNING LIGHT - CONTROL | ?????
5 | 0.5 | 26LC | COLUMN STATUS SIGNAL 2 | ?????
7 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
8 | 0.5 | 14M | WINDSCREEN WIPER PARK POSITION CONTROL > COMPUTER | ?????
10 | 0.5 | 26N | ENGINE START/STOP + SIGNAL | ?????
11 | 0.3 | 5DU | GEAR LEVER LOCKING - CONTROL | ?????
12 | 0.5 | 26LB | COLUMN STATUS SIGNAL 1 | ?????