| FRONT WIRING
H45/BVVR/2TR

#### 1337
SWITCHING PROTECTION UNIT
DG/TR4X2/SSESP/NINAV4/RAD04,RAD05,RAD07

5 | 1.2 | AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE | ?????
6 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL | ?????
7 | 1.2 | 3FB | INJECTION + > PROTECTIVE RELAY | ?????
8 | 1.2 | 85D | 4X4 TORQUE CONTROL | ?????
10 | 0.5 | 85G | 4X4 CLUTCH RELAY CONTROL | ?????
1 | 0.5 | APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST | ?????
2 | 1.2 | 3BS | IGNITION COIL CONTROL | ?????