| FRONT WIRING
H45/BVM6/2TR

#### 226
RIGHT-HAND HEADLIGHT
DD/TR4X4/SSESP/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 0.5 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
2 | 0.5 | 11S | RIGHT-HAND PROTECTED SIDE LIGHT +CONTROL | ?????
4 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
5 | 0.85 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT + | ?????
6 | 0.85 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
7 | 0.85 | RPD | RIGHT HAND PROTECTED MAIN BEAM HEADLIGHT + | ?????
8 | 0.85 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????