Norton Commando Workshop Manual

## Frame and Ancillaries

# F

6 | Fit the shims and end cap to the mounting with the thickest shim to the cap.
7 | In order to refit the gaiter, polyurethane washer, and collar, the gaiter must be held back as far as possible on the lip of the collar, as shown in Fig. F5 to gain sufficient room for fitting.

| If it proves extremely difficult to insert the parts, have a second operator push the rear wheel as far as possible from right to left, thus providing maximum clearance at the end of the rear mounting.
8 | After entering the end cap, gaiter etc. ensure that the gaiter fits completely over the mounting and cap without being trapped at either end. Check then that the collar, polyurethane washer etc. are free to revolve with the gaiter.

<< | < | rocbo.net | >