## Fan Controls

#### Symptom Troubleshooting Index

10-14

Before performing any troubleshooting procedures check:

- Fuses
- Grounds
- Cleanliness and tightness of all connectors

  SYMPTOM | PROCEDURE
  Radiator fan does not run at all | Radiator Fan Circuit Troubleshooting (see page 10-16).
  Radiator fan does not runs for engine cooling, but it runs with A/C on | Radiator Fan Switch Circuit Troubleshooting (Open) (see page 10-18).
  Radiator fan runs with ignition switch ON (II), A/C off and engine temperature below 93oC (199oF) | Radiator Fan Switch Circuit Troubleshooting (Short) (see page 10-18).