## Torque Converter Housing

#### Mainshaft Bearing and Oil Seal Replacement

14-190

Special Tools Required

- Adjustable bearing remover set, 07JAC-PH80000
- Handle driver, 07749-0010000
- Driver attachment, 62 x 68 mm, 07746-0010500
- Driver attachment, 72 x 75 mm, 07746-0010600

1. Remove the mainshaft bearing and oil seal with the special tool.

2. Install the new mainshaft bearing until it bottoms in the housing with the special tools.

3. Install the new oil seal flush with the housing using special tools.