## Engine Assembly

#### Engine Installation (cont'd)

5-17

22. Install the A/C compressor (A), then install the alternator lower bracket (B).

23. Install the A/C hose bracket.

24. Loosely install the alternator.
25. Adjust the alternator belt, refer to the '01 Civic Shop Manual on this CD (see page 4-38).
26. Push the ECM/PCM connectors through the bulkhead, then install the grommet (A).

RHD models:

LHD models:

27. Install the harness clamps (B).