## Manual Transmission

#### Output Shaft Reassembly

13-25

Exploded View

NOTE: Before assembling, apply oil to the thrust surface of all gears, bearing interior and race surfaces.

1. Front output shaft bearing
2. Rear output shaft bearing, 3rd and 4th output gear
3. 3rd and 4th gear feather key
4. 2nd gear needle bearing
5. Output 2nd gear
6. 2nd block ring set
7. 2nd gear needle bearing collar, 1st and 2nd synchroniser assembly, output 1st gear
8. 1st and 2nd synchroniser assembly
9. 1st block ring set
10. Output 1st gear
11. 1st block needle bearing
12. 1st thrust bearing
13. Output shaft

a a a